Atlas Copco DM30,year:2014,hours:Zero

Part Lists:

**1-Insulated, pressurized, with colored glass cabs with suspended seats.**

**2-1050CFM @ 100PSI air compressor, 29.7M ^ 3 / min @ 7.6 bar**

**3-Caterpillar C15 diesel engine, 540HP @ 1800RPM**

**4-Caterpillar excavator chassis, three-tooth track**

**5-Hydraulic cylinder driven wire rope feed system**

**6-The hydraulic motor drives the rotary head**

**7-Remote control hydraulic drill lock pin**

**8-The battery pack jumps up**

**9-Hydraulic drive rod holder, can accommodate 127mm drill pipe 4**

**10-No impact switch**

**11-Hydraulic calipers**

**12-Auxiliary hydraulic chain clamp**

**13-2700kg auxiliary winch**

**14-Hydraulic retractable dust curtain**

**15-Three strokes of 1.2m leveling jack**

**16-Cooling device: divided into four parts, respectively, hydraulic oil, air compressor oil, engine coolant (52 degrees Celsius)**

**17-Separate air compressor and diesel engine intake filter**

**18-The main frame of the wide - edge steel structure with balanced beam**

**19-11x halogen lamps (70W)**

**20-Maintenance channel with guardrail**

**21-Traffic warning**

**22-Jack retract indicator light**

**23-Engine preheating device**

**24-Hydraulic oil heater**

**25-Air compressor tank preheater (requires 220V AC power supply)**

**26-Radiator heater (requires 220V AC power supply)**

**27-Angle drilling 0 ° -30 °**

**28-A set of O-rings, a set of maintenance tools**

**29-Dry dust collector**

**30-Central lubrication system**

**31-Cab hot and cold air conditioning**

**32-230 gallon fuel tank**

**33-Automatic thread lubrication (pneumatic)**

**34-Torque limiting device**

**35-Walking, rotary interlocking device**