# 1、Project Installation：

1. ), Installation Instruction (PDF/WORD file): free charge.
2. ), Sending Technician: The client affords all fees include the round trip air ticket/hotel/food/wage.

# 2、Area calculation rules:

1. )、Room area: Length x Width （㎡）.
2. )、Canopy area: half of the canopy horizontal projection area （㎡）. Total area is: 1)+2).

**3**、**Quotations:** Date: OCT.11, 2017

|  |
| --- |
| **Quotation: Prefab House School and Toilet (75mm color steel EPS sandwich panel**） |
|  | **Description** | **Dimension of per classroom** | **Pic** | **Area**㎡ | **TTL Area Per Unit**㎡ | **Unit** | **Unit Price usd/unit (FOB)** | **Total Amount USD (FOB)** | **REMARK** |
| 1 | K-type 5 classrooms | 45.70\*6.57M (L x W) |  | 300.25 | 323.10 | 5 | $17,800.00 | $91,000.00 | 3P\*3.5K\*25K,1unit with 5 classrooms. |
| K-type 5 classrooms canopy | 45.70\*1M/2 (L x W) |  | 22.85 | 1 unit canopy in 1 building (5 classrooms) |
| 2 | K-type toilet | 5.66\*5.66M (L x W) |  | 32.03 | 34.86 | 1 | $2,950.00 | $2,950.00 | 3P\*3K\*3K |
| K-type toilet canopy | 5.66\*1M/2 (L x W) |  | 2.83 |
| 3 | Moisturepr oof partitionboard | for squatting pot |  |  |  | 10 sets | $95.00 | $950.00 | include the door for each sqatting pan |
| Squatting Pan Sets |  |  |  |  | 10 sets | $45.00 | $450.00 | include the water tank,triangular valve and |
| Staniless steel Urinal slot | 3.6 m |  |  |  | 1 | $580.00 | $580.00 | Men's room |
| Pedestal Basin |  |  |  |  | 2 sets | $38.00 | $76.00 | include the faucet |
| Indoor water supply and drainage | include pipe connector and accessories |  |  | 1 | $675.00 | $675.00 | for toilet |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 4 | Housing installation tools |  |  | 1 sets | $650.00 | $650.00 | Optional |
| 5 | indoor electricity distributions | wire、switchs、socket、 lamps |  | 1650.36m2 |  | $6.80/m2 | $11,222.45 | for all classrooms and toilet. |
| Total amount include tool (FOB): | $106,653.45 |  |

**Remark:**

1, Price term: FOB FUZHOU, CHINA.

2, Payment Term: 50% TT deposit, balance 50% TT paid before delivery. 3, Lead time: within 30 days after receive the 50% T/T deposit.

4, Quotation Expiry Date: OCT. 26, 2017.

5, The above price is only for the house body and the items listed, does not include foundation, installation and other items unlisted in the above quotation sheet.

|  |
| --- |
| **Material Specifications of K-type prefab house (dimensions tolerance:0~±5%)**： |
| 1、Pillar：C100\*1.8 mm section steel； |  |
| 2、Roof Purline/Ring Beam：L40\*2.0mm angle steel； |  |
| 3、Roof Truss：C60\*1.5mm + 口40\*30\*1.0mm Square tube combination； |  |
| 4、Ground beam： C100\*1.8 mm section steel； |  |
| 5、Outer wall panel：75mm double color steel (0.25mm) EPS sandwich panel； |  |



|  |  |
| --- | --- |
| 6、Inner wall panel：75mm double color steel (0.25mm) EPS sandwich panel； |  |
| 7、Roof Panel：75mm double color steel (0.25mm) EPS corrugate sandwich panel； |  |
| 8、Door：Steel sandwich panel door； |  |
| 9、Window/Shutter ：PVC sliding widows； |  |

Design drawing of 5 classrooms:

Design drawing of Toilet:

