

|  |
| --- |
|  |
| **Quotation for 36m2 Foam Cement House** |
| **PRICE DETAIL** |
| NO. | PART | DESCRIPTION | QUANTITY | UNIT |  |  |
| **Cement House Main Body** |
| 1 | Mainbody | Cement House Main Body | 36 | M2 |  |  |
| **Doors and Windows** |
| 2 | Doors | Steel Security Door for Entrance（D1） | 1 | SET |  |  |
| Composite Wood Door for Bedroom(D2) | 3 | SET |  |  |
| Windows | Aluminum Sliding Window W1 | 4 | PCS |  |  |
| Aluminum Sliding Window W2 | 1 | PCS |  |  |
| **Total Doors and Windows Price** |  |
| **Decoration Materials** |
| 3 | Floor Decoration | Cermic Tile | 96 | PCS |  |  |
| **Total Decoration Price** |  |
|  |
| DESCRIPTION | QUANTITY | UNIT |  |  |
| 4 | 40'HQ Qingdao Port Inland Shipping and Port Charges | 2 | Container |  |  |
| Total Inland Shipping and Port Charges |  |
|  |  |
|  | **House Design Draw** |
| 5 |  |
| 6 | Payment Terms | 100% T/T before loading |
| 7 | Validity of Quotation | 15 days |
| 8 | Shipping | By Sea, the Loading Port, Qingdao, China |
| 9 | Packing | 1\*40'HQGP containers can load 2 unit of this house with all above |
| 10 | Size | SPEC: 6.6m\*5.4m\*2.8m |
| **Materials List** |
| **No.** | **PART** | **First Part (Main Part of House)** | **Material** | **Specification** | **Quantity** | **Unit** | **Picture** |
| 1 | Mainbody Panel | 94mm External Wall Panel | Foamed Cement Panel | 8mm Fiber Cement Board on two surface; 78mm thickness Foam Cement Core; Build-in Steel Structure | 73.1 | M2 |  |
| 2 | 94mm Internal Wall Panel | 35.3 | M2 |
| 3 | 94mm Roof Panel | 44.9 | M2 |
| 4 | Structure to Fix Pane | Square Tube(Using for Basement,Use Expansion Bolt to fix it,then Wall Panel sit on the Square Tube) | Square Tube | 30mm\*30mm\*2mm | 36.6 | M |  |
| 5 | Square Tube (Using for Ring Beam to strength the Whole Steel Structure) | Square Tube | 30mm\*30mm\*2mm | 25.8 | M |  |



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6 | Panel Gap Painting | Plaster for External Wall | White | 11.5m2 Use One Bag | 10 | BAG |  |
| 7 | Plaster for Internal Wall | 12 | BAG |
| 8 | Sealing Tape for Gap Fixing | White | Standard | 23 | PCS |  |
| 9 | Undercoat | Standard | Standard | 27 | KG |  |
| 10 | `Beam | A-Beam | Hot Galvanized Steel 5400m(Length) | L50\*50\*3 | 2 | PCS |  |
| 11 | Roof | Glazed tile | Galvanize Steel | 828mm\*0.5mm | 57.6 | M |  |
| 12 | Ridge tile | 0.5mm | 7.5 | M |  |
| **NO.** | **PART** | **Second Part (Doors and Windows)** | **Material** | **Specification** | **Quantity** | **Unit** | **Picture** |
| 1 | Doors | Steel Security Door for Entrance | Steel | 960mm\*2050mm (W\*L) | 1 | SET |  |
| 2 | Composite Wood Door for Bedroom | Wood | 860mm\*2050mm (W\*L) | 2 | SET |  |
| 3 | Aluminum Alloy Door | Aluminum Alloy | 750mm\*2050mm (W\*L) | 1 | SET |  |
| 4 | Windows | Aluminum Sliding Window(white and single glass) | Aluminum Alloy | 1140mm\*1300mm (L\*W) | 6 | PCS |  |
| 6 | 1140mm\*900mm (L\*W) | 1 | PCS |
| 7 | 540mm\*900mm (L\*W) | 1 | PCS |
| **NO.** | **PART** | **Third Part (Decoration Materials)** | **Material** | **Specification** | **Quantity** | **Unit** | **Picture** |
| 1 | Floor Decoration | Ceramic Tiles for Internal Floor | Ceramic Tile | 600mm\*600mm\*10 mm(L\*W\*T) | 96 | PCS |  |
| Note: This offer for current materials market; The Price is not including installation expenses |
|  |
| **2018-6-19** |