|  |
| --- |
|  |
|  |
| **Quotation of Easy Folding Container House** |
| **Loading Quantity** | **Quantity** | **Unit** | **FOB Price** | **Total FOB Amount** |
| 10 Units per 40'HQ | 10 | Unit | **USD1950** | **USD19,500** |
| **Dimension** |
| External Dimension (mm) | 5800 L \* 2500 W \* 2560H |
| Internal Dimension (mm) | 5660 L \* 2360 W \* 2350H |
| Folding Dimension (mm) | 5800 L \* 2500 W \* 430H |
| Total Weight (kg) | 1200 |
| **Standard Design Parameter** |
| No. | Item | Technical Data |
| 1 | Roof Load | ≧0.5KN/m2 |
| 2 | Flooring Load | ≧2.0KN/m2 |
| 6 | Fire-proof Level | A Level |
| 8 | Seismic Grade | 8 Grade |
| 9 | Windproof Level | 10 Level |
| **Main Materials** |
| **No.** | **Component** | **Materials** | **Thickness (mm)** |
| **Steel Structure** |
| 1 | Hanging Head | 200\*80mm, Cast steel connecting piece | 15 |
| 2 | Column | 150\*150mm, Special-shaped galvanized steel | 1.5 |
| 3 | Bottom Frame | H:270mm,Special-shaped galvanized steel | 2.5 |
| 4 | Top Frame | H:170mm,Special-shaped galvanized steel | 1.5 |
| 5 | Hinge | 85\*115 mm，Galvanized 304 stainless steel | 5 |
| **Wall Panel & Roof Tile** |
| Roof | External Roof | Corrugated steel plate | 0.45 |
| Interior Roof | Ceiling tile 0.35mm, glass wool 75mm |  |
| Floor | Floor | MGO board | 15.0 |
| Wall | Interior Wall Panel | Galvanized color steel plate | 0.3 |
| External Wall Panel | Galvanized color steel plate | 0.3 |
| Sadnwich Wall Panel | Fireproof rock wool board | 50.0 |
| **Window & Door&Floor** |
| 1 | Door | High quality security door | 860\*1998 |
| 2 | Window | Aluminum alloy window | 950\*1200×2 |
| **Electrical System** |
| Voltage | 220V~250V |
| Wire | The total power cord for entry is 6.0 square meters, the air conditioning cable is 4.0 square meters, the socket cable is 2.5 square meters, and the lighting switch cable is 1.5 square meters |
| Circuit Breaker | high score break miniature circuit breaker |
| Lighting | 1 set of single LED fluorescent lamps,36w |
| Sockets | socket, 3 pcs |
| **Remark: the quotation is valid until Aug. 30th, 2024** |