|  |
| --- |
| CONDITION OF SALE / SPECIAL INSTRUCTIONS:This will be provided under separate cover. |
| PRODUCT: OXYGEN CONCENTRATORS - 5L | APPLICATION: Medical |  |
| SALESPERSON | P.O. NUMBER | SHIP DATE | SHIP VIA | F.O.B. POINT | DELIVERY TERMS |
| Gerald Provost | TO BE PROVIDED | TBD | BUYER LOGISTICS | China - Outgoing port could be Shanghai, Shenzhen, GuanZhou or Hong Kong. | PER | CUSTOMER  |
|  |
| QUANTITY | DESCRIPTION | UNIT PRICE  | IMAGE | AMOUNT |
| 2000 | 5L OXYGEN CONCENTRATOR (MODEL:8F-5AW)POWER SOURCE：AC220V±22V，50Hz±1HzRATED POWER：350WNOISE：＜58dB（A）FLOW RANGE：1-5L/minOXYGEN PURITY：1-5L/min≥90%MAX OUTPUT PRESSURE：45KPa±4.5KPaCOMPRESSOR PROTECT PRESSURE：250KPa±25KPaFLOW FLUCTUTION（UNDER BACK PRESSURE 7KPa）：0.7L/minNEBULIZER FLOW：≥0.2mL/minCONTINUOUS RUNNING TIME：24HOURSCURRENT OVERLOAD PROTECTION SWITCH：5A，220VPRODUCT WEIGHT：22 KgENVIRONMENT TEMPERATURE：5℃~40℃HUMIDITY RANGE：≤80%ATMOSPHERIC PRESSURE RANGE：86KPa~106KPaOCSI TEMPERATURE AND ATMOSPHERIC PRESSURE RANGE：0~50℃；150KPaOXYGEN PURITY WHEN ALERT FROM OCSI：＜82%±1.5%（80.5%~83.5%）ALTITUDE IN USING：USE UNDER THAN 1,828MCERTIFICATIONCurrently being used WHO and Red Cross | $734.40 |  |  |
|  |  |  |  |  |
| SUBTOTAL TAX RATE SALES TAX OTHER  |  |
|  |
|   |
|   |
|  |
| THANK YOUFOR YOUR BUSINESS |
|  |
|  PROSPECTIVE CUSTOMER  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name Managing Principal Title |