

**Quotation for expandable container house**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | | | | |
| **No** | **item** | **specification** | **picture** | **loading quantity** | **price** |
| 1 | DRF-1 | **open room with steel door** 1)openable size 5850mm\*6085mm\*2500mm Closed size: 5850mm\*2250mm\*2500mm) 2)75mm eps sandwich panel for wall and roof  3)16mm reinforced MGO board+1.6mm pvc tile for floor 4)with 1 steel  door(930\*2030mm), 8 pvc double glazed sliding windows  （930\*930mm);  5)with electricity, DB box, switch, sockets, A/C sockets, wires, etc.; |  | 1\*40HC container can load 2 units | **DISCOUNT**  **PRICE:USD7,700/**  **UNI T EXW** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 2 | DRF-2 | **open room with sliding door** 1)openable size 5850mm\*6085mm\*2500mm Closed size: 5850mm\*2250mm\*2500mm) 2)75mm eps sandwich panel for wall and roof  3)16mm reinforced MGO board+1.6mm pvc tile for floor 4)with 1 aluminum hinged door door(W1300\*H2000mm),8 pvc double glazed sliding windows  （930\*1130mm);  5)with electricity, DB box, switch, sockets, A/C sockets, wires, etc.; |  | 1\*40HC container can load 2 units | **DISCOUNT PRICE:USD7,990/**  **UNIT EXW** |
| 3 | DRF-3 | **Open Space with a Toilet Layout**  1)openable size 5850mm\*6085mm\*2500mm Closed size: 5850mm\*2250mm\*2500mm) 2)75mm eps sandwich panel for wall and roof  3)16mm reinforced MGO board+1.6mm pvc tile for floor 4)with 1 aluminum double glazed hinged door(W1300\*H2000mm), 8 pvc double glazed sliding windows  （930\*930mm), 1 bathroom exhaust fan ;   1. with electricity, DB box, switch, sockets, A/C sockets, wires, etc.; 2. with bathroom(shower   ,shower tray,seat toilet,wash basin,plumbing) |  | 1\*40HC container can load 2 units | **DISCOUNT PRICE**  **USD8,810/UNIT EXW** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4 | DRF-4 | **1 Bedroom Layout** 1)openable size 5850mm\*6085mm\*2500mm Closed size: 5850mm\*2250mm\*2500mm) 2)75mm eps sandwich panel for wall and roof  3)16mm reinforced MGO board+1.6mm pvc tile for floor 4)with 1 aluminum double glazed hinged door(W1260\*H2000mm), 8 pvc double glazed sliding windows  （930\*930mm), 1 bathroom exhaust fan ;   1. with electricity, DB box, switch, sockets, A/C sockets, wires, etc.; 2. with bathroom(shower   ,shower tray,seat toilet,wash basin,plumbing)   1. with one bedroom 8)with 1.8m long kitchen |  | 1\*40HC container can load 2 units | **DISCOUNT PRICE**  **USD8,979/UNIT EXW** |
| 5 | DRF-5 | **2 Bedroom Layout** 1)openable size 5850mm\*6085mm\*2500mm Closed size: 5850mm\*2250mm\*2500mm) 2)75mm eps sandwich panel for wall and roof  3)16mm reinforced MGO board+1.6mm pvc tile for floor 4)with 1 aluminum double glazed hinged door(W1260\*H2000mm), 8 pvc double glazed sliding windows  （930\*930mm), 1 bathroom exhaust fan ;   1. with electricity, DB box, switch, sockets, A/C sockets, wires, etc.; 2. with bathroom(shower   ,shower tray,seat toilet,wash basin,plumbing)   1. with two bedrooms 8)with 1.8m long kitchen |  | 1\*40HC container can load 2 units | **DISCOUNT**  **PRICE:USD8,999/**  **UNIT EXW** |
| **remark** | | | | | |

|  |
| --- |
| **payment terms:50% deposit by T/T,50% balance before shipment** |
| **valid time:in 7 days** |
| **lead time:45 days** |
| **one 40HC container can load 2 units** |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **material list for expandable container house with bathroom and kitchen** | | | | | | | | | |
| **Project name:** | | | | | | | **Project No.:** | | |
| **Specification:** | | |  | **5850mm\*6085mm\*2500mm** | | | **Area:** | **35.5** | **m2** |
| **NO** | **ITEM** | | **SPECIFICATION** | | **UNIT** | **QUANT ITY** |  |  | **PICTURE** |
| 1 | middle frame**( our frame is thicke r than others**  **)** | top main beam | | 120\*42\*5mm thickness channel beam welded 60\*2.3mm steel plate and 135\*25\*40\*2.3mm channel |  |  |  |  |  |
| 2 | corner | | the same size as shipping container,8.6KG/P CS |  |
| 3 | bottom secondary beam | | 100\*50\*1.5mm galvanized tube steel |  |
| 4 | top secondary beam | | 40\*60\*1.5mm and 30\*30\*1.5mm galvanized tube steel |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 5 |  | bottom main beam | bended galvanized steel 2.3mm thickness | SET | 1.0 |  |  |  |
| 6 | column | bended galvanized steel 2.3mm thickness |  |
| 7 | two sides frame**( our frame is thicke r than others**  **)** | roof frame | bended galvanized tube steel 77\*50\*1.8mm |  |
| 8 | wall frame | bended galvanized tube steel 77\*50\*1.8mm |  |
| 9 | floor frame | 100\*50\*1.5mm and 50\*50\*1.5mm galvanized tube steel |  |
| 10 | other access ories | hook and hinges | steel |  |
| 11 | wall**(ot her comp any's wall is just 50mm**  **)** | exterior | 75mm eps sandwich panel,outer skin 0.4mm,10KG/M3 |  |  |  |  |  |
| 12 | interior | 50mm eps sandwich panel,outer skin 0.4mm,10KG/M3 |
| 13 | roof**(ot her comp** | roof of expandable part | 75mm eps sandwich panel,outer skin 0.4mm,10KG/M3 |



|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 14 | **any's**  **roof is just 50mm**  **)** | roof of main part | 0.4mm thickness steel sheet+50mm eps sandwich panel | SET | 1.0 |  |  |  |
| 15 |  | acceossorie s | edge cover,bolt sealant |  |
| 16 | floor | sub floor | 15mm thickness MGO board |  |
| 17 |  | surface floor | 1.6mm thickness pvc floor tile |
| 18 |  | electricity | DB box, switch, sockets, A/C sockets, wires, etc |  |
| 19 | windo w | pvc sliding window double glazed | 8pcs 930\*930mm |  |
| 20 | door | exterior | aluminum hinged door double glazed 1260\*2000mm |  |
| 21 | plumbi ng | pre-installed | | SET | 1.0 |  |  |  |
| 22 | bathro om partitio n |  | sandwich panel+one door+extra corner decoration | set | 1.0 |  |  |
| 23 | glass showe r cabin |  |  | set | 1.0 |  |  |  |
| 24 | toilet | ceremic seat toilet | universal standard | set | 1.0 |  |  |




|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 25 | wash basin | with faucet etc accessories | universal standard | set | 1.0 |  |  |  |
| 26 | kitche n | with bottom cupboard,st ainless  steel countertop | 1.8m long | set | 1.0 |  |  |  |
| 27 | bedroo m partitio n | 75mm eps sandwich panel | double skin 0.4mm,10KG/M3 | set | 1.0 |  |  |  |
| 28 |  | |  |  |  |  |  |  |
| 29 | **Subtotal** | | EXW | | | | **8,999** |  |





Furniture NOT included



**drawing**

