**Cargo Freighter Specifications**

B737-300F






Payload-Range


Loading Specification




Main Deck

Lower Deck


ULD Reference

Refer to above Main Deck (Orange Color)

or

Refer to above Main Deck (Green Color)

Refer to above Main Deck (Light Blue Color)

or


|  |  |
| --- | --- |
| Payload (Tons) | 15,000 to 18,000 |
| Volume (cbm) | 130 |
| Main Door Dimension (LxH, cm) | 350x230 |
| Forward Door Dimension (LxH, cm) | 122x130 |
| After Door Dimension (LxH, cm) | 124x122 |
| Max Range (km) | 3,028 |
| Cruise speed (km/h) | 820 |
| MTOW (kg) | 63,276 |
| MZFW (kg) | 49,714 |
| Crew & Cargo Attendants | 2 |
| Max fuel capacity (kg) | 20,100 |
| Average fuel burn (tons/h) | 2.6 |
| Minimum runway (m) | 2,280 |