|  |
| --- |
| **√Model：ADICKZ6720K**  |
| **SPECIFICATION**  |
| Dimension (mm) | 7235\*2050\*2650 | Kerb/Gross weight (kg) | 4500/7000 |
| Max Speed (km/h) | 100 | App/Dep(O) | 17/13 |
| Wheel Track (mm) | 1830/1650 | Wheel Base (mm) | 3935 |
| Engine  | See below | Seat Capacity | 1 +24 (+ 5 Folding) |
| Steering | Power Steering | Seat type | Fabric seat |
| Clutch  | Single, Dry, Diaphragm | Rearview Mirror | Manual, |
| Transmission  | 5 forward+1 reverse | Passenger door | Manual |
| Brake | (See below) | Suspension | Leaf spring  |
| Tire | 7.00R16 | A/C | Optional |
| Others:  | Tinted Glasses, Fire Extinguisher, Mp3 Radio  |
| **Petrol Bus: Engine: JM495QF-III** **Toyota engine. 2693CC. Hydraulic Brake****Ex Factory USD25999** |
| **Diesel Bus: Engine 1): CY4102-E3C AIR BRAKE**  **Ex Factory 25500****Engine2): EQB125-20 Cummins, Air Brake****Ex Factory USD25999** |
| Optional List | RHD: cost rise $400， air condition kcal add cost USD2500;  |

