|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | |  | | | 5.5 x 5.0 m (27.5m2)  dispensary TENT(IFRC/ICRC type)  specifications | | |  | | | Size  Height  Wall Height  Doors  Windows  Frame  Accessories  Ground Sheet  Mud Flaps  Material  Rain Fly (optional)  Product Key  Features: | 5.5 x 5.0 m  2.50 m  1.80 m  One door on each gable end with opening/closing system.  4 windows with mosquito nets and rolled flaps.  Powder coated metal frame with steel connectors.  One tent packed with all standard accessories in bales & wooden crates.  PVC coated fabric 2 sides coated, weight: 540 gsm. (+/-10%)  PVC coated fabric 2 sides coated, weight: 540 gsm (+/-10%).  Roof, wall fabric: Poly-Cotton blended fiber yarns, 440 gsm in finished state. Waterproof and Rotproof.  PVC coated Fabric of 550 gsm (+/-10%).  • Dispensary tent which can be used for clinic, health center, storage or temporary shelter purposes and can be extendable to one another to make a longer structures.  • Separate ground sheet for use in tent is available as an option in case main tent is used for living / clinics. | |  | |  | | --- | | quick DEPLOYABLE tentideal for schools, office, health center, storage and TEMPORARY group shelters.suitable for clinics and medical usetent has the bath tub shape ground sheet to protect from insects and water | |  | | **PRICE: US$ 1,290/- per tent (FOB Lahore Airport)**  **Stock Quantity: 30 tents**  **Delivery: Immediate** | |