Manufacturer: Boeing Max Taxi Weight: 250,998 lbs / 113,851 kg

Model: B757-200PCF Max Gross Take-Off Weight: 249,999 lbs / 113,398 kg

Max Landing Weight: 209,999 lbs / 95,254 kg

Max Zero Fuel Weight: 185,999 lbs / 84,368 kg

Operators Empty Weight: 117,050 lbs / 53,093 kg

Date of Manufacture: 1991 Payload: 68,000 lbs / 30,844 kg

Current Location: USA

Range with Full Payload: 4,000 NM / 7,408 km

Airframe Life Limit: 150,000 hours or 75,000 cycles

TSN: 81,185 Hours CSN: 30,109 Cycles

Landing Gear

Main Landing Gear (LH) M0735N0362 12,467 25,160 3,855 Oct 2022

Main Landing Gear (RH) M0736N0362 12,467 46,592 3,855 Oct 2022

Nose Landing Gear M0607N0601 12,467 24,955 3,855 Oct 2022