# 

# QUOTATION

**Description: Electric Pick-up Car**

**Model NO.: TBIPT-320 2022**

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
| Controller | 60V Intelligent Controller | Motor | 3000W Alternator |
| Storage Battery | 12V\*5PCS,100AH | Traveling Range | 90-120km |
| Battey charger | Vehicle-mounted Intelligent Charger | Charging Time | 8-10Hours |
| Charger Voltage | Single phase,220V | GW | 700 KGS |
|  | | | |
| Overall Size | 3200\*1450\*1700mm(L\*W\*H) | Body&Chassis Material | Metal |
| Carriage Box Size | 1530\*1350\*300mm(L\*W\*H) | Loading Capacity | 600 kgs |
| Speed Range | 40-45km/h | Braking Length | ≤ 7 Meters |
| Climbing Capacity | 25-30% | Min.Turning Tadius | 7500 MM |
| Wheel Base | 1330 MM | Front and Rear Tracks | 1360 MM |
|  | | | |
| Seat Material | Imitation leather (PU) | | |
| Instrument Panel | Combined Instrument（front/back signal,light,trumpet,dump energy,current speed display） | | |
| Lighting System | Combined type front light and back light,braking light,front/back turning light | | |
| Switch System | Light switch,main power switch,electric horn,wiper switch. | | |
| Entertainment System | Digital LCD panel, MP3 Player,USB Port,Backup Camera | | |
| Car Body Painting | Color can be customized. | | |
|  | | | |
| Drive System | Rear-drive motor,Controller adjusted automatically | | |
| Steering System | Automatic adjustment rack and pinion direction | | |
| Braking System | Four wheel hydraulic brake + double circuit hydraulic brake + parking brake device + brake assist | | |
| Tire Details | 145-70/R12, Steel wheel hub, Vacuum tire | | |
| Front Axle and Suspension | Integral front bridge suspension | | |
| Back Axle and Suspension | Integral front bridge suspension | | |
|  | | | |
| **FOB QINGDAO** | **USD 5,200 / SET With 2 Seats,2 Doors and A/C is included.** | | |

1. **Warranty:** One years warranty for the electric car, replacement parts can be offered for free during warranty, lifelong time after sales service.
2. **Payment Terms:**

50% Prepayment by T/T to start produce ,balance paid before loading container.

1. **Package Info:** By seaworthy case, or by steel plate, then loading by container.
2. **Delivery Time:** Within 30 days after getting 50% prepayment.
3. **Validity:** The quotation is valid within 20 days.

