|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CONDITION OF SALE / SPECIAL INSTRUCTIONS:  This will be provided under separate cover. | | | | | |
| PRODUCT: OXYGEN CONCENTRATORS - 5L | APPLICATION: Medical | | |  | | |
| SALESPERSON | P.O. NUMBER | SHIP DATE | SHIP VIA | F.O.B. POINT | DELIVERY TERMS |
| Gerald Provost | TO BE PROVIDED | TBD | BUYER LOGISTICS | China - Outgoing port could be  Shanghai, Shenzhen, GuanZhou or Hong Kong. | PER | CUSTOMER |
|  | | | | | |
| QUANTITY | DESCRIPTION | | UNIT PRICE | IMAGE | AMOUNT |
| 2000 | 5L OXYGEN CONCENTRATOR (MODEL:8F-5AW)  POWER SOURCE：AC220V±22V，50Hz±1Hz  RATED POWER：350W  NOISE：＜58dB（A）  FLOW RANGE：1-5L/min  OXYGEN PURITY：1-5L/min≥90%  MAX OUTPUT PRESSURE：45KPa±4.5KPa  COMPRESSOR PROTECT PRESSURE：250KPa±25KPa  FLOW FLUCTUTION（UNDER BACK PRESSURE  7KPa）：0.7L/min  NEBULIZER FLOW：≥0.2mL/min  CONTINUOUS RUNNING TIME：24HOURS  CURRENT OVERLOAD PROTECTION SWITCH：5A，220V  PRODUCT WEIGHT：22 Kg  ENVIRONMENT TEMPERATURE：5℃~40℃  HUMIDITY RANGE：≤80%  ATMOSPHERIC PRESSURE RANGE：86KPa~106KPa  OCSI TEMPERATURE AND ATMOSPHERIC PRESSURE  RANGE：0~50℃；150KPa  OXYGEN PURITY WHEN ALERT FROM  OCSI：＜82%±1.5%（80.5%~83.5%）  ALTITUDE IN USING：USE UNDER THAN 1,828M  CERTIFICATION  Currently being used WHO and Red Cross | | $734.40 |  |  |
|  |  | |  |  |  |
| SUBTOTAL  TAX RATE  SALES TAX  OTHER | | | | |  |
|  |
|  |
|  |
|  |
| THANK YOU  FOR YOUR BUSINESS |
|  | | | | | |
| PROSPECTIVE CUSTOMER    \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Name  Managing Principal Title | | | | | |