

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | | | |
| SPEC  **G2 VEHICLE SPEC** | | | |
|  | | | | |
| **Product Name** |  | **Terriitori G2 Passenger Electrical Vehicle JEEP** | | |
| **Item** | | **Specification** | **Reference Pictures** | |
| **Overall Size** | | 3300×1600mm×1700mm |  | |
| **steering wheel** | | LHD(Left side steering wheel)&RHD |
| **Seats Capacity** | | 4 Seats |
| **Curb Weight** | | 645Kg(with battery) |
| **Engine Power** | | 60V4000W Motor 60V 4000W |
| **Battery** | | 60V 103AH, Lead acid Battery Recommend |
| **Controller** | | Special Controller |
| **Charger Type** | | Vehicle-mounted |
| **Driving Mode** | | Rear Mounted / Rear Drive |
| **Damping system F** | | Integrated Front Axle + longitudinal arm torsion beam Non-independent suspension |
| **Damping system R** | | Integrated Axle + longitudinal arm torsion beam Non-independent suspension |
| **Car Body Structure** | | Frame type+ Stamping |
| **Display Instrument** | | Liquid Crystal Electronic Digital Display 7 Inch +MP5 |
| **Brake System** | | F Disc / R Disc |
| **Brake Type** | | Pedal Oil Brake |
| **Tyre** | | 165/70R 12 Vacuum Tires |
| **Wheel Hub** | | Iron hub + cover |
| **Maximum Speed** | | 50 Km/H |
| **Charging type& Time** | | China type, 8~10Hours (General) |
| **Endurance Mileage** | | about 100-120km |
| **Driving&Copilot Seats** | | Manual Adjusted Seats, Two Directions |
| **Headrest** | | not adjustable |
| **Central Lock** | | Yes with Remote key |
| **Intelligent Remote Key** | | Yes |
| **Cooling System** | | with air conditioner |
| **Security System** | | Backup Camera +MP5 |
| **Entertainment System** | | MP5 Multimedia Player, Stereo Speaker MP5 |
| **Light Combination** | | ①LED Headlamp,LED ②Standalone Steering Lamp, ③Taillight,④ High-mount Stop Lamp, |
| **Other Configuration** | | ①Windshield Wiper, ②Power Windows, ③Folding & Adjustable Rearview Mirror |
| **Color options** | | ①White ② Red ③Blue ④Pink |
| **Container Load** | | CBU 4 Sets in 40HQ |
| **Shipment Port** | | Qingdao/Shanghai/Lianyungang Port |
| **Remarks** | | \*1. About this Quotation, Barring special circumstances, the above quotations valid in 15 workdays.  \*2. About Packaging, Standard export packing, or customized packing as your request  \*3. About Payment, By T/T: 50% amount in advance, 50% amount paid before delivery.  \*4. About Delivery time, Based on actual quantity, 25 working days in general after payment receipt confirmed.  \*5. About Quality Guarantee,12 months for Main Parts, include motor/controller/frame/battery. | | |

( Please sign back when confirmed )