Details are listed below:

|  |  |  |
| --- | --- | --- |
| **DESCRIPTION** | **UNIT** | **QTY.Available** |
| GLOBE CONTROL VALVE (Actuated) 8" 600# RF. Body Mat.: A890 Gr 4A (UNSS31803) | EA | 1 |
| GLOBE CONTROL VALVE  (Actuated) 4" 600# RF.Body Mat.: A216 WCC | EA | 2 |
| GLOBE CONTROL VALVE  (Actuated) 1 1/2" 600# RF. Body Mat.: A351 CF8M | EA | 1 |
| GLOBE CONTROL VALVE  (Actuated) 10" 600# RF. Body Mat.: A890 Gr 4A (UNSS31803) | EA | 2 |
| GLOBE CONTROL VALVE  (Actuated) 8" 600# RF.Body Mat.: A216 WCC | EA | 3 |
| GLOBE CONTROL VALVE  (Actuated) 14" 600# RF.Body Mat.: A216 WCC | EA | 2 |
| PRESSURE CONTROL VALVE(Actuated) 1" 150# RF. Body Mat.: A216 WCC | EA | 1 |
| PRESSURE CONTROL VALVE(Actuated) 1" 150# RF. Body Mat.: A216 WCC | EA | 1 |
| SPARE PARTS | EA | 1 |
| CHECK VALVE PISTON 1 1/2" 800#SW. Body Mat.: A105. type: Bolted Cover, Pison Lift | EA | 2 |
| CHECK VALVE WAFER 3" 150# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 150# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 15 |
| CHECK VALVE WAFER 4" 150# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 2 |
| CHECK VALVE PISTON 3/4" 800# THD.Body Mat.: A105. type: Bolted Cover, Pison Lift | EA | 2 |
| CHECK VALVE WAFER 3" 150# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 2 |
| CHECK VALVE PISTON 2" 800# THD.Body Mat.: A105. type: Bolted Cover, Pison Lift | EA | 2 |
| CHECK VALVE WAFER 3" 150# RF.Body Mat.: A351 CF8M. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 150# RF.Body Mat.: A351 CF8M. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 600# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 600# RF.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 600# RF.Body Mat.: A351 CF8M. Type: Wafer Lug/Dual Plate | EA | 2 |
| CHECK VALVE WAFER 2" 600# RF.Body Mat.: A890 Gr.4A. Type: Wafer Lug/Dual Plate | EA | 3 |
| CHECK VALVE WAFER 2" 900# RTJ.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 2 |
| CHECK VALVE WAFER 2" 900# RTJ.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 1 |
| CHECK VALVE WAFER 2" 900# RTJ.Body Mat.: A216 WCB. Type: Wafer Lug/Dual Plate | EA | 2 |
| BLOW DOWN VALVE (Actuated) 3"600# RF. Body Mat.: A350 LF2 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"600# RF. Body Mat.: A350 LF2 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"900# RTJ. Body Mat.: A350 LF2 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"900# RTJ. Body Mat.: A350 LF2 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"900# RTJ. Body Mat.: A350 LF2 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"900# RTJ. Body Mat.: A182 F316 | EA | 1 |
| BLOW DOWN VALVE (Actuated) 2"900# RTJ. Body Mat.: A182 F316 | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 3" 150# RF. Body Mat.: A350 LF2. SERVICE CLASS B | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 3" 150# RF. Body Mat.: A182 F316. SERVICE CLASS B | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A350 LF2. SERVICE CLASS B | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 2" 900# RTJ. Body Mat.: A350 LF2. SERVICE CLASS B | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 1 1/2" 150# RF. Body Mat.: A350 LF2. SERVICE CLASS B | EA | 1 |
| MOTORIZED VALVE (Actuated) 3" 150#RF. Body Mat.: A350 LF2. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A350 LF2. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A350 LF2. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A350 LF2. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A350 LF2. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 150# RF. Body Mat.: A182 F316. | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 2" 600# RF. Body Mat.: A182 F316. | EA | 1 |
| ON-OFF VALVE (Actuated) 2" 150# RF.Body Mat.: A350 LF2. | EA | 1 |
| BALL VALVE (Manual) 2" 900# RTJ.Body Mat.: A350 LF2. Data sheet: BFG01J1 | EA | 2 |
| BALL VALVE (Manual) 3/4" 1500# Puppiece PE 100 mm long. Body Mat.: A350 LF2. Data sheet: BFG01N1 | EA | 2 |
| BALL VALVE (Manual) 2" 900# RTJ.Body Mat.: A182 F316. Data sheet: BFG49J1 | EA | 1 |
| BALL VALVE (Manual) 2" 900# RTJ.Body Mat.: A182 F316. Data sheet: BRG49J1 | EA | 2 |
| PROCESS SHUT DOWN VALVE(Actuated) 8" 300# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: D | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 8" 300# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: D | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 8" 300# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: D | EA | 1 |
| BALL VALVE (Manual) 4" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 LF51. Service class: D | EA | 6 |
| BALL VALVE (Manual) 2" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: D | EA | 5 |
| BALL VALVE (Manual) 3" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: D | EA | 4 |
| GLOBE VALVE (Manual) 6" 600# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A995 Gr.A. | EA | 1 |
| GLOBE VALVE (Manual) 3" 150# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB | EA | 1 |
| GLOBE VALVE (Manual) 2" 150# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB | EA | 8 |
| GLOBE VALVE (Manual) 2" 150# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB | EA | 2 |
| GLOBE VALVE (Manual) 2" 150# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A351 CF8M | EA | 1 |
| GLOBE VALVE (Manual) 2" 600# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB | EA | 9 |
| GLOBE VALVE (Manual) 2" 600# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB. Weld Overlay | EA | 13 |
| GLOBE VALVE (Manual) 2" 600# RF.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A351 CF8M | EA | 1 |
| GLOBE VALVE (Manual) 1/2" 800# SW.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A182 F316L | EA | 2 |
| GLOBE VALVE (Manual) 2" 900# RTJ.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB. Weld Overlay | EA | 1 |
| GLOBE VALVE (Manual) 2" 900# RTJ.Type: OS&Y, Bolted Bonnet, Swivel Plug Disc. Body Mat.: A216 WCB. NACE | EA | 1 |
| DUAL PLATE CHECK VALVE 20" 150#RF. Body Mat.: A216 WCB. Data sheet: CDB03R1 | EA | 1 |
| GLOBE CONTROL VALVE (Actuated)10" 600# RF. Body Mat.: A890 Gr 4A (UNSS31803) | EA | 1 |
| BLOW DOWN VALVES (Actuated) 4"600# RF. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. | EA | 1 |
| BLOW DOWN VALVES (Actuated) 4"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. | EA | 1 |
| BLOW DOWN VALVES (Actuated) 6"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. | EA | 1 |
| BLOW DOWN VALVES (Actuated) 4"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A182 F316. | EA | 1 |
| EMERGENCY SHUT DOWN VALVE.(Actuated) 10" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE.(Actuated) 10" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE.(Actuated) 8" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE.(Actuated) 10" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE.(Actuated) 10" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 16" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 16" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 4" 150# RF. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2.Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 6" 150# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 12" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 4" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 18" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 14" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 12" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 6" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 16" 900# RTJ. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 16" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 16" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 4" 150# RF. Type:BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 4" 150# RF. Type:BALL. Bore type: FULL. Body Mat.: A182 F318. Service class: B | EA | 2 |
| BALL VALVE (Manual) 4" 600# RF. Type:BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 14" 600# RF.Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| BALL VALVE (Manual) 8" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 3 |
| BALL VALVE (Manual) 6" 600# RF. Type:BALL. Bore type: FULL. Body Mat.: A182 F51. Service class: B | EA | 6 |
| BALL VALVE (Manual) 4" 600# RF. Type:BALL. Bore type: FULL. Body Mat.: A182 F51. Service class: B | EA | 4 |
| BALL VALVE (Manual) 10" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 F316LN. Service class: B | EA | 3 |
| BALL VALVE (Manual) 8" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 F316LN. Service class: B | EA | 4 |
| BALL VALVE (Manual) 10" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 F51. Service class: B | EA | 1 |
| BALL VALVE (Manual) 12" 600# RF.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 14 |
| BALL VALVE (Manual) 16" 600# RF.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 5 |
| BALL VALVE (Manual) 6" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 4" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 2 |
| BALL VALVE (Manual) 4" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 4 |
| BALL VALVE (Manual) 12" 600# RF.Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 12 |
| BALL VALVE (Manual) 10" 600# RF.Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 3 |
| BALL VALVE (Manual) 6" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 2 |
| BALL VALVE (Manual) 10" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 0 |
| BALL VALVE (Manual) 16" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 2 |
| BALL VALVE (Manual) 4" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 3 |
| BALL VALVE (Manual) 8" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 2 |
| BALL VALVE (Manual) 10" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 2 |
| BALL VALVE (Manual) 8" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A182 F51. Service class: B | EA | 1 |
| BALL VALVE (Manual) 10" 150# RF.Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 900# RTJ.Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| SPARE PARTS AND CONSUMABLES FOR START-UP AND COMMISSIONING FOR ON-OFF VALVES | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 20" 600# RF. Type: BALL. Bore type: REDUCED. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 150# RF. Type:BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 300# RF. Type:BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 3 |
| BALL VALVE (Manual) 4" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 600# RF. Type:BALL. Bore type: REDUCED. Body Mat.: A182 F351. Service class: B | EA | 1 |
| BALL VALVE (Manual) 6" 900# RTJ.Type: BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 3 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 1/2" SW (extended inlet). Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A216 WCB | EA | 5 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 2" 1500# RTJ. Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A216 WCB | EA | 27 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 2" 1500# RTJ. Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A216 WCB | EA | 43 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 1/2" SW (extended inlet). Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A182 F51 | EA | 18 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 1/2" SW (extended inlet). Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A182 F316L | EA | 6 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 1" SW (extended inlet). Outlet: 1" SW. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: A182 F316L | EA | 3 |
| DOUBLE BLOCK  & BLEED VALVE.Inlet: 2" 1500# RTJ. Outlet: 1/2"  NPTF. Bleed: 1/2" NPTF needle valve w/plug. Body Mat.: UNS S31803 | EA | 70 |
| DOUBLE BLOCK  & BLEED VALVE. Inlet: 2" 1500# RTJ. Outlet: 2" 1500#RTJ. Bleed: 1/2" NPTF needle valvew/plug. Body Mat.: A182 F51 | EA | 2 |
| Surch (Value)(Head) | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 10" 900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 2" 1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: E | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 10" 900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 1" 1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 1 |
| BLOW DOWN VALVES (Actuated) 2"1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A182 F51. Service class: B | EA | 1 |
| BLOW DOWN VALVES (Actuated) 3"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| BLOW DOWN VALVES (Actuated) 2"1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A352 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 1" 1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 1 |
| BLOW DOWN VALVES (Actuated) 3"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| PROCESS SHUT DOWN VALVE(Actuated) 1" 1500# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A182 F316. Service class: B | EA | 1 |
| BLOW DOWN VALVES (Actuated) 3"900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: B | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| SPARE PARTS AND CONSUMABLESFOR START-UP | EA | 1 |
| EMERGENCY SHUT DOWN VALVE(Actuated) 10" 900# RTJ. Type: BALL. Bore type: FULL. Body Mat.: A350 LF2. Service class: E | EA | 1 |

**Condition:**

Unused. Original packing from the manufacturer.