## 


## Electric Car Quotation Description: Right Hand Drive Electric Car

**Model: TBIEC-340**

**2024**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **EC340-128KM** | **EC340-220KM** | **EC340 -Fast Charge** |
| **Vehicle Body Size L\*W\*H (mm)** | 3444\*1550\*1535 | | |
| **Wheel Base (mm)** | 2350 | | |
| **Wheel Track (mm)** | 1360/1342 | | |
| **Climbing Capacity（%）** | ≥25% | ≥25% | ≥30% |
| **Ground Clearance (mm)** | 180 | | |
| **Maximum Speed（km/h）** | 100km/h | | |
| **Maximum Traveling Range ( km )** | 128km | 219km | 210km |
| **Driver Position** | Left hand steering | | |
| **NO.of Seats** | Four seats/ 3 doors | | |
| **Location of Charging Port** | Front Grille,Built in Type | | |
| **FOB PRICE** | | | |
| **FOB QINGDAO** | **USD 7500** | **USD 8500** | **USD 8800** |
| **Motor Information** | | | |
| **Motor Power (KW)** | Front/rated 2KW Peak 4KW; Rear/rated 12KW Peak 25KW | | |
| **Motor Type** | AC Motor | | |
| **Driving Type** | 4WD | | |
| **Minimum Turning Diameter** | ≤9.5m | | |
| **Ready Quality/Full Load Quality** | 840kg/1100kg | | |
| **Battery Information** | | | |
| **Battery Type** | Li battery | | |
| **Battery Capacity** | 10.24KW/h | 18.43KWh | 17.9km/h |
| **Number of Battery** | 1 | | |
| **Normal Charge Times（hr）** | 4h | 8h | 1h |
| **Chassis & Steering** | | | |
| **Front Suspension Type** | Mcpherson Independent Suspension | | |
| **Rear Suspension Type** | Trailing-Arm | | |
| **Body Type** | Unibody | | |
| **Brake System & Wheels** | | | |
| **Front Brake Type** | Disc Brake | | |
| **Rear Brake Type** | Drum Brake | | |
| **Steering Gear** | EPS | | |
| **Tyre Size** | 175/55R15 | | |
| **Wheel Hub Type** | Aluminium alloy | | |

|  |  |
| --- | --- |
| **Safety Configuration & Driving Assistance** | |
| **ABS** | ● |
| **EPS** | ● |
| **Rear View Camera** | ● |
| **Safety Belt** | Front/ Rear |
| **Tire Pressure Monitoring** | ● |
| **Rear Parking Radar** | ● |
| **Driving Mode Selection** | Economy/sports |
| **Uphill Aid** | ● |
| **Automatic Driving Lock** | ● |
| **Roof Rack** | ● |
| **Roof Trunk** | ○ |
| **Roof Lights** | ● |
| **Car Central Control Lock** | ● |
| **Remote Key** | ● |
| **Keyless Start Function** | ● |
| **The Luggage Compartment Opens** | ● |
| **Interior Collocation** | |
| **All-liquid Crystal Instrument** | ● |
| **Liquid Crystal Instrument Dimensions** | 5 Inch |
| **Seat Material** | PU |
| **Main/passenger Seat Adjustment** | Anteroposterior adjustment/ Backrest adjustment |
| **Steering Wheel Material** | PU |
| **Lamp Configuration** | |
| **Daytime Running Lamps** | ● |
| **Steering Lamp** | ● |
| **Fog Light** | ● |
| **Clearance Lamp** | ● |
| **Combination Headlight** | ● |
| **Combination Tail Lamp** | ● |
| **High brake light** | ● |
| **Reversing Light** | ● |
| **Multimedia & Air-conditioning** | |
| **Multimedia Touch Screen** | 9 Inch |
| **Local Video Player** | ● |
| **Local Music Player** | ● |
| **Radio** | ● |
| **Phone Charging Interface** | ● |
| **Bluetooth Music/ Phone** | ● |
| **Mobile Internet** | ● |
| **Mobile Wifi** | ● |
| **GPS** | ● |
| **USB** | 2 |
| **Multilingual Menu Operation** | ● |
| **Air-Conditioning** | ● |



### Color Option



### Front Front Side



**Front Side Rear**



**Side Side**



### Dash Board Streeing Wheel



**Gear Switch Display Screen**



**PU Seats Trunk**



|  |  |  |
| --- | --- | --- |
| **LCL (Less Than Container Load) if only one sample required add $1,000 this will be deductible when you place MOQ order** | | |
| **Package Size:** |  | **Gross Weight:** |
| **Package Way** |  | Fixed inside steel frame,then covered with plywood. |



|  |  |  |
| --- | --- | --- |
| **Full Container Loading** | | |
| **20 ft container** |  | **40 ft container** |
| **Package Way** |  | Fixed by steel frame,then fixed on the container ground with nylon tape. |

