****

**QUOTATION**

**Description: Four Wheel Electric Mini Car**

**Model NO.: TBIA-520 2024**

|  |  |
| --- | --- |
| **Electrial System** | |
| Controller | 60V Intelligent Controller |
| Storage Battery | 12V\*5PCS,80 AH |
| Motor Power | 2200 W |
| Traveling Range | 80-100km |
| Battey charger | On board Charger |
| Charger Voltage | Single phase,220V(110V) |
| Charging Time | 8-10Hours |
| GW | 380 KGS |
| **Technicial Data** | |
| Overall Size | 2500\*1202\*1625mm(L\*W\*H) |
| Seating Capacity | 2-3 Seats/ 2 Doors |
| Speed Range | 25km/h or 45km/h |
| Climbing Capacity | 25% |
| Body Material | Injection molding plastic |
| Chassis Material | Metal |
| Braking Length | ≤ 5 Meters |
| Min.Turning Tadius | 8500 MM |
| Rear Tracks | 1000 MM |
| Wheel Base | 1742 MM |
| **Car Body System** | |
| Steering System | **Handle steering** |
| Seat Material | Imitation leather (PU) |
| Instrument Panel | Combined Instrument（front/back signal,light,trumpet,dump energy,current speed display） |
| Lighting System | Combined type front light and back light,braking light,front/back turning light |
| Switch System | Light switch,main power switch,electric horn,wiper switch. |
| Entertainment System | Digital LCD panel,Radio,USB Port,Speaker, Bluetooth,Backup Camera,Built-in Antenna |
| Car Body Painting | Color can be customized. |
| Safety Performance | Hill assist,Safety belts,Remote control key, Electric window, Warm wind,Sky window. |
| **Chassis System** | |
| Drive System | Rear-drive motor,Controller adjusted automatically |
| Braking System | Disk Brake |
| Wheel Details | Front: 125/65 R12, Rear: 135/70 R12, Aluminium alloy. |
| Vehicle Structure | Load-supporting body frame |
| Front Suspension | MacPherson independent suspension |
| Rear Suspension | Trailing arm drive axle |
| **FOB PRICE** | |
| **FOB QINGDAO** | **USD 3200 / SET ( MOQ 10 SETS)**  **USD 3100 / SET (11-100 SETS) USD 2950 / SET (101 ≤ SETS)** |

1. **Warranty:** One years warranty for the electric car, replacement parts can be offered for free during warranty, lifelong time after sales service.
2. **Payment Terms:**

50% Prepayment by T/T to start produce, balance paid before loading container.

1. **Package Info:** By seaworthy case, or by steel plate, then loading by container.
2. **Delivery Time:** Within 20 days after getting 30% prepayment.
3. **Validity:** The quotation is valid within 20 days.



**Front Front-left**



**Side Side**



**Rear Rear-right**



**Cockpit Instrument**



**Gear Switch Panoramic Sunroof**



**Front Seats Load-supporting Frame**



|  |  |  |  |
| --- | --- | --- | --- |
| **LCL (Less Than Container Load) if only one sample required add $1,000 this will be deductible when you place MOQ order** | | | |
| **Package Size:** | 2600\*1300\*1800mm | **Gross Weight:** | 450 kgs |
| **Package Way** | Fixed inside steel frame,then covered with plywood. | | |



|  |  |  |  |
| --- | --- | --- | --- |
| **Full Container Loading** | | | |
| **20 ft container** | 2 pcs | **40 ft container** | 9 pcs |
| **Package Way** | Fixed by steel frame,then fixed on the container ground with nylon tape. | | |

