

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | |
| **To:** | |  | | | **Invoice No.** | TBIRH2024031401 |
| **Address:** | |  | | | **Date:** | 2024.03.14 |
|  | |  | Email: |  |  |  |
|  | | | | | | |
|  | | | | | | |
| TBI J2-P with EEC L7e BU | | | | | | |
| **No**  **.** | **Model with standard** | | | **FOB unit** | **QTY(Unit)** | **Totally** |
| 1 | TBIJ2-P Electric Vehicle  （206Ah LiFePo4 Battery with BMS & Fast charging system +5000W Motor） | | | $8,000.00 | 8 | $64,000.00 |
| 2 | Iron package frame | | | $100.00 | 8 | $800.00 |
| Optional Items & price | | | | | | |
| 1 | 105Ah LiFePo4 Battery Battery with BMS& Fast charging system (3-5 hours) | | | -1500 USD |  |  |
| 2 | Air conditioner | | | +430 USD |  |  |
| 3 | Hopper 1635\*1150\*370mm | | | -300USD |  |  |
| 4 | Insulation box 500\*40\*30mm | | | +25 USD |  |  |
| 5 | Cargo box with cooling system -5℃ | | | +500 USD |  |  |
| 6 | Cargo box with cooling system -18℃ | | | +600 USD |  |  |
| 7 | 4000W Motor | | | -300 USD |  |  |
| 8 | Rear Disc Brake | | | +50 USD |  |  |
| 9 | Fan | | | +30 USD |  |  |
| 10 | 1:8 rear axle for high speed（Max speed 60km/hour） | | | +90USD |  |  |
| 11 | Solar panel | | | +500 USD |  |  |
| 12 | Trailer hook | | | +100USD |  |  |
| 13 | Swivel Driver's Seat | | | +100USD |  |  |
|  | **Total FOB Qingdao Price** | | | | | **$** |
| Not e | 1.The price is based on FOB Qingdao price.And the rate between USD to RMB is subject to 1USD≈7.10CNY. | | | | | |
| 2.Payment Term: 50% advance payment, the balance will be paid before delivery. | | | | | |
| 3.Delivery Time: 30 days after receive the advance payment. | | | | | |
| 4.Packing: MOQ 4 units for 1\*40GP, 8Units for 1\*40HQ. | | | | | |
| Standard Configuration | | | | | | |
| **No**  **.** |  | **Item** | | | **J2-P** | |
| 1 | **Parameter** | L\*W\*H （mm) | | | 3600\*1345\*1765 | |
| 2 | Wheel Base(mm) | | | 2375 | |
| 3 | Min.Ground Clearance (mm) | | | 160 | |
| 4 | Curb Weight（kg） | | | 500 | |
| 5 | Max. Speed(km/h) | | | 52 | |
| 6 | Max. Range (km) | | | 160 | |
| 7 | Capacity (person) | | | 1 | |
| 8 | Cargo Box Size(mm) | | | 1635\*1150\*1058 | |
| 10 | Rated Load(kg) | | | 550 | |
| 11 | Steering Mode | | | Middle Steering Wheel | |
| 12 | **Power System** | A/C Motor | | | 60V 5000W | |
| 13 | Lithium Battery | | | 206Ah LiFePo4 Battery | |
| 14 | Charhing Time | | | 4-6 hrs (220V) | |
| 15 | Charger | | | Intellengent Charger | |
| 16 | **Brake System** | Type | | | Hydraulic System | |
| 17 | Front | | | Disc | |
| 18 | Rear | | | Disc | |
| 19 | **Suspension System** | Front | | | Independent Double Wishbone | |
| 20 | Rear | | | Integrated Rear Axle | |
| 21 | **Wheel Suspension** | Tyre | | | Front 135/70-R12 Rear145/70-R12 | |
| 22 | Wheel Hub | | | Aluminum Alloy Hub | |

|  |  |  |  |
| --- | --- | --- | --- |
| 23 | **Function Device** | Mutil-media | MP3+Reverse Camera |
| 24 | Electric Heater | 60V 800W |
| 25 | Central Lock | Auto Level |
| 26 | One Button Start | Auto Level |
| 27 | Electric Door & Window | 2 |
| 28 | Skylight | Manual |
| 29 | Seats | Leather |
| 30 | Kindly Note that all configuration is only for your reference in accordance with EEC homologation. | | |
|  | | | |
| 1 |  | | |